Home > Network > Additional Methods of Configuring Your Lenovo Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™ > How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

### How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

Related Models:M7206W / M7216NWA / M7256WHF

1. Press MENU.
2. Press or to select the Network option, and then press OK.
3. Press or to select the WLAN option, and then press OK.
4. Press or to select the WPS/AOSS option, and then press OK.
5. When WLAN Enable? appears, enable the wireless network.
   This will start the wireless setup wizard.
6. When the LCD shows Press Key on rtr, press the WPS or AOSS™ button on your wireless access point/router. Then press OK and your machine will now automatically detect which mode (WPS or AOSS™) your wireless access point/router uses and try to connect to your wireless network.

If your wireless device is connected successfully, the machine's LCD displays Connected. The machine will print your machine's wireless status report. If the connection fails, check the error code on the printed report.
(For models with wired network function) If the connection fails, your machine reverts to a wired network interface.

For Windows®:

You have completed the wireless network setup. To install drivers and software necessary for operating your device, click Multi-Function Suite Install on the Installer CD-ROM's Install Software page.

For Macintosh:

You have completed the wireless network setup. Go to the Lenovo Website at http://www.lenovo.com to install drivers and software necessary for operating your device.

Related Information
  - Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™
  - Wireless LAN Report Error Codes

Go to top of page