[Boot]
Caption              = "WinSail V2.0演示程序"
GotoMonitor=0
Switch               = Off

EnglishVersion       = Off

XmsStyle             = 1
Icon                 = "bmp\Sail2000.Ico"
TouchUser=1

[Comm]
CommBase=COM1
IPAddress=13361
OtherAddress         =13361
MotorNet             =1
IdleNet=False
PC386                =False
CommDelay            =False
SendFileAfterWait    =200
SendFilePageWait     =300
CommWaittingTime     =-1L;3000000L
Baud=4800

[Display]
;Font = "Font\GBK_K.Fon"
;Display.Fon"
Device=11
Mode=117
Mono=False
Freq=0

;Syntax = Device, Mode, Colors, DriveName
BGI=

[Debug]
DebugState           =Off
SafetyDescription    =Off
Comm                 =Off
DoorMonitor          =Off


[Print]
Caption1       = "            ";
Caption2       = " =======================";
Caption3       = "FS-200型智能电枢测试系统";
RecordRow      = 35;//24
ExtraWidth     = 65;Uint Is Character
Printer        = LPT1;\\Yao\Epson 740

[SpcPassword]
user01=Super ,88888888
user02=User  ,88888888
user03=Normal,88888888

[System]
MultiTask = False

TestTimes=1
JudgeRight=1
Buzzer=1
Speaker=0
DialogBox=1
Continue=1

[Netcard]
NetCard=1

HostName=oemcomputer
My_IP=169.254.82.133

PeerName=NT-Server
you_IP=169.254.210.218

NetMask=255.255.0.0
Gateway=169.254.1.1

NameServer=

[Ime]
Ime1 = Ime\Winqp.ime
Ime2 = Ime\Winwb86.ime
Ime3 = Ime\GBK_pq1.ime
Ime4 = Ime\GBK_pq2.ime

[End]
