;
; Roland Modela configuration file 
;
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; BEM 13/05/94 Modified header to remove @ command
; TM  07/02/96 Modified - added pause command
; TM  07/02/96 Modified - Additional XY feedrates
; JAB 21/06/99 Modified for the Modela, half resolution
; TM  25/11/99 Modified to use steps of 0.25mm
; BEM 09/06/00 Added Description and file extension fields
; BEM 15/06/00 Changed to match test file from Joules
;
DESCRIPTION = "Roland Modela (Alpha Test) (*.rol)"
;
FILE_EXTENSION = "rol"
;
; Set units used in file - MM
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
;
; Roland use mm/s for output feed rate so divide by 60
; this is ame as * (1/60)
;
FORMAT = [F|@||1.1|0.0166]
;
; Tool moves in x,y and z
;
; Roland uses positions in 0.01 of a mm on CAMM3
; On the Modela they use 0.025 of a mm.
;
FORMAT = [X|@||1.0|40]
FORMAT = [Y|@||1.0|40]
FORMAT = [Z|@||1.0|40]
; Home tool positions 
FORMAT = [XH|@||1.0|40]
FORMAT = [YH|@||1.0|40]
FORMAT = [ZH|@||1.0|40]
;
; Set up program header
;
; Initialise
;
START = ";;^IN;"
;
; Switch on the spindle
;
START = "!MC1;"
;
; Start moving at rapid rate
;
START = "V15.0;"
;
; Relative move x0,y0 Z upto maximum height ? - presumably a safety move
;
START = "^PR;Z0,0,1626;"
;
; Set Absolute mode
;
START = "^PA;"
;
; Set feed rate used for rapid moves 15mm/s = 900mm/min
;
RAPID_FEED_RATE = 900
;
; Set up data output on change of feed rate
;
FEED_RATE_CHANGE = "V[F];"
;
; Program moves
;
FEED_RATE_MOVE  = "Z[X],[Y],[Z];"
;
; End of file - go home and stop spindle
;
END = "!MC0;"
