;
; MaxNC configuration file 
;
;
; History
;
; Who When     What
; === ======== ========================================
; MA  22/09/94 Feed rate variable edited to enable both F and E to be used.
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; ejp 30/05/02 Modified from Model Master for rotary axis
; bem 30/08/02 mirror y (output as X !) to allow for rotation
; ejp 30/05/02 Modified for Model Master with 'true' rotary axis
; bem 13/09/04 Changed naming convention AND changed mapping
;              of Axis so that X no longer reversed
; ejp 06/10/04 Also map Y to X so that we can set the Y home 
; tls 23/03/05 Modified to run MaxNC Rotary 
; bmd 10/05/05 Modified to run 3 axis Max CNC desktop
;
DESCRIPTION = "Max_NC_Metric (*.T)"
;
FILE_EXTENSION = "T"
;
UNITS = MM
;
;
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y,z and r
FORMAT = [X|#| X |1.3]
FORMAT = [Y|#| Y |1.3]
FORMAT = [Z|#| Z |1.3]
;FORMAT = [R|#| A |1.4|-1.0]
; Home tool positions 
FORMAT = [XH|@| X |1.3]
FORMAT = [YH|@| Y |1.3]
FORMAT = [ZH|@| Z |1.3]
;FORMAT = [RH|@| A |1.4|-1.0]
;
; Set up program header
;
START = "([TOOLPATHNAME])"
START = "G90G80G49G21"
START = "G00[XH][YH]"
START = "M03 [S]"
START = "G00[ZH]"
START = "G41D6"
;
; Program moves
;
FIRST_RAPID_RATE_MOVE  = "G00 [X][Y][Z]"
RAPID_RATE_MOVE        = "G00 [X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G01 [X][Y][Z] [F]"
FEED_RATE_MOVE         = "G01 [X][Y][Z]"
;
; End of file
;                          
;END = "G0 [RH]"
END = "G00[ZH]"
END = "M30"
END = "M99"
;
