;
; Isel NCP format configuration file 
;
; History
;
; Who  When        What
; ===  =========== ==============================================
; GJO  09/04/2001  Modified for use with Galaad-KAY interface
; TM   11/08/2003  Added Tool number
;
DESCRIPTION = "isel (*.ncp)"
;
FILE_EXTENSION = "ncp"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Block numbering 
;
LINE_NUM_START      = 10
LINE_NUM_INCREMENT  = 1
LINE_NUM_MAXIMUM    = 99999
LINE_NUM_INC_ON_USE = 1
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|06.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#| VEL |1.0|15.00]
; Tool moves in x,y and z
FORMAT = [X|#| X|1.0|1000.0]
FORMAT = [Y|#| Y|1.0|1000.1]
FORMAT = [Z|#| Z|1.0|1000]
;
; Home tool positions 
FORMAT = [XH|#| X|1.0|1000]
FORMAT = [YH|#| Y|1.0|1000]
FORMAT = [ZH|#| Z|1.0|1000]
;
; Set up program header
;
START = "1MF_PBL_V1.0"
START = ";**********************************"
START = ";Type:    Alcami Soloutions"
START = ";Machine: Isel from Unimatic soloutions"
START = ";**********************************"
START = " FASTVEL 40000"
START = " INITTOOL"
START = " SPINDLE OFF"
START = " COOLANT OFF"
START = " GETTOOL [T]"
START = " SPINDLE RPM[S]"
START = " SPINDLE ON"
START = " WAIT 2000"
START = " FASTABS[XH][YH]"
START = " FASTABS[ZH]"
START = " COOLANT ON"
;
FEED_RATE_CHANGE = "[F]"
;
RAPID_RATE_MOVE        = " FASTABS[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = " MOVEABS[X][Y][Z]"
;
; Program moves
;
FEED_RATE_MOVE = " MOVEABS[X][Y][Z]"
;
; End of file
END = " FASTABS[Z]"
END = " FASTABS[X][Y]"
END = " SPINDLE OFF"
END = " COOLANT OFF"
END = " PROGEND"