 ;
 ; Holz-Her _____-master configuration file - Code Configuration File
 
 ; History
 ;
 ; Who When     What
 ; === ======== ========================================
 ; MEF 10/9/02  Modified for Metroplex Cabinet Holz-Her 327 Router.
 ; MEF 10/30/02 ADDED PROGRAM, MODIFED USER VARIABLES, ADDED G120 LINE.
 ; MEF 10/31/02 ADD VARIABLE TO PROPERTIES SET TO 1 FOR INCH, 0 FOR METRIC.
 ; MEF 12/19/02 TO READ PROGRAMS LARGER THAN 64K A SEPARATE PROGRAM MUST CALL SUBPROGRAM (M98 K"XXXX" R1) 
 ; MEF 12/19/02 WHERE XXXX = MAIN PROG. R1 = NUMBER OF REPEATS.
 ; MEF 12/19/02 FILES MUST BE IN C:\MW310\PROG\ FOLDER.
 ; MEF 12/19/02 SPINDLE SPEEDS MUST BE DEFINED IN TOOL LIBRARY AS 2 DIGITS ONLY, i.e. S14 = 14000 rpm
 ; mef 12/19/02 Changed format for Z to reverse signs.
 ; bmd 09/29/05 Modified to run Holz-Her Ecomaster 7120
 ; jvg 03/26/07 will run all twinCAM Holz-Her's; Eco-Master, Easy-Master, Union-Master		
 ;
 DESCRIPTION = "Holz-Her -Master TC(*.TWN)"
 ;
 FILE_EXTENSION = "TWN"
 ;
 UNITS = MM
 ;
 ; Cariage return - line feed at end of each line
 ;
 END_OF_LINE = "[13][10]"
 ;
 ; Block numbering 
 ;
 LINE_NUM_START     = 0010
 LINE_NUM_INCREMENT = 10
 LINE_NUM_MAXIMUM   = 99999999
 ;
 ; Set up default formating for variables
 ;
 ; Line numbering
 FORMAT = [N|@|N|1.0]
 ; Spindle Speed
 FORMAT = [S|@||1.0]
 ; Feed Rate
 FORMAT = [F|#|F|1.0]
 ; Tool moves in x,y and z
 FORMAT = [X|#|X|1.3]
 FORMAT = [Y|#|Y|1.3]
 FORMAT = [Z|#|Z|1.3]
 ; Home tool positions 
 FORMAT = [XH|@|X|1.3]
 FORMAT = [YH|@|Y|1.3]
 FORMAT = [ZH|@|Z|1.3]
 ;
 ;
 ; Set up program header
 ;
 ;
 START = ""
 START = ";#PANEL X[XSIZE]  Y[YSIZE]  Z[ZMATERIAL]"
 START = ";ZONE AF"		
 START = "; ArtCAM Pro  Software"
 START = "[N] TC_CHANGETOOL([T][44]1[44]3[44][S][44][44][44][44][44][SZ][44][44])"
 START = "[N] TC_SETFACE(0)"
 START = "[N] ATRANS X0 Y0 Z0"
 START = "[N] TC_SETFACE(0)"
 START = ";START ROUTING SEQUENCE [TOOLDESC] TOOL [T]"
 START = "[N] TC_CHANGETOOL([T][44]1[44]3[44][S][44][44][44][44][44][SZ][44][44])"
 START = "[N] G0 [XH] [YH] M61"
 START = "[N] G0 [ZH]"
 START = "[N] TC_STARTKONTUR"
 ;
 ;
 ; Program moves
 ;
 RAPID_RATE_MOVE        ="[N] G0 [X] [Y] [Z] [F]"
 FIRST_FEED_RATE_MOVE   ="[N] G1 [X] [Y] [Z] [F]"
 FEED_RATE_MOVE         ="[N] G1 [X] [Y] [Z]"
 ;
 ;
 ; Toolchange moves (only output for 2nd and later tools)
 ;
 ;
 TOOLCHANGE = "[N] TC_ENDKONTUR(0)"
 TOOLCHANGE = "[N] TC_CHANGETOOL([T][44]1[44]3[44][S][44][44][44][44][44][SZ][44][44])"
 TOOLCHANGE = "[N] TC_STARTKONTUR"
 ;
 ;
 ; End of file
 ;
 ;
 END = "[N] TC_ENDKONTUR(0)"
 END = "[N] G0 [ZH]"
 END = "[N] M60"
 ;