;
; Osai configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 18/11/97 Written
; Andrea Amilo - Delcam Italia - 22/09/05
;
;
DESCRIPTION = "Osai Biesse H1RT (*.iso)"
;
FILE_EXTENSION = "iso"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 1
LINE_NUM_INCREMENT = 1
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@||1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.0]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
; Arc Centre Cordinates
FORMAT = [IA|@|I|1.3]
FORMAT = [JA|@|J|1.3]
;
MIN_ARC_LENGTH = 0.05
;
; Set up program header
;
START = ";HEAD1 RIGHT TABLE"
START = ";"
START = "[34]START[34]"
START = "G90 G71"
START = "G0 G79 Z0."
START = "G0W0Y0"
START = "M500 M5 M20M91"
START = "M100"
START = "M700 M22 M9"
START = "G0 G79 Z0."
START = "P2850"
START = "M0"
START = "P2850"
START = "(DAN)"
START = "G16 XY"
START = "(UAO,1)"
START = "(UTO,1,X50,Y50,Z50)"
START = ";[TOOLDESC]"
START = "M500 M5 M20"
START = "G0 G79 Z0"
START = "(AXO,-Z)"
START = "M91"
START = "T[T].[T] M6"
START = "M501"
START = "M92"
START = "M10"
START = "M3 [S]"
START = "G0[XH] [YH]"
START = "G0[ZH]"
;
; Archi
;
FIRST_CW_ARC_MOVE      = "G2[X][Y]R[Radius][F]"
CW_ARC_MOVE            = "G2[X][Y]R[Radius]"
;
FIRST_CCW_ARC_MOVE     = "G3[X][Y]R[Radius][F]"
CCW_ARC_MOVE           = "G3[X][Y]R[Radius]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[X][Y][Z][F]"
;
;

TOOLCHANGE = "M20"
TOOLCHANGE = "M5"
TOOLCHANGE = "M91"
TOOLCHANGE = ";[TOOLDESC]"
TOOLCHANGE = "M500 M5 M20"
TOOLCHANGE = "G0 G79 Z0"
TOOLCHANGE = "(AXO,-Z)"
TOOLCHANGE = "M91"
TOOLCHANGE = "T[T].[T] M6"
TOOLCHANGE = "M501"
TOOLCHANGE = "M91"
TOOLCHANGE = "M10"
TOOLCHANGE = "M3 [S]"
TOOLCHANGE = "G0[XH] [YH]"
TOOLCHANGE = "G0[ZH]"
;
;

END = "M20"
END = "M5"
END = "M91"
END = "M500"
END = "G0 G79 Y0. Z0."
END = "[34]SUBOUT[34]"
END = "M30"
;
