;
; Bostomatic configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; bjs 02/07/97 WRITTEN  atg
; bem 16/05/00 Modified 
;
DESCRIPTION = "Bostomatic Incremental (*.tap)"
;
FILE_EXTENSION = "tap"
;
UNITS = INCH
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
;LINE_NUM_START     = 0
;LINE_NUM_INCREMENT = 1
;LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
;FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [XI|#|X|1.0|10000]
FORMAT = [YI|#|Y|1.0|10000]
FORMAT = [ZI|#|Z|1.0|10000]
; Home tool positions 
FORMAT = [XH|@|X|1.0|10000]
FORMAT = [YH|@|Y|1.0|10000]
FORMAT = [ZH|@|Z|1.0|10000]
;
; Set up program header
;
START = "%"
START = "G91"
START = "T1"
START = "G1M04R"
;
; Program moves
;
RAPID_RATE_MOVE        = "G1[XI][YI][ZI]R"
FIRST_FEED_RATE_MOVE   = "G1[XI][YI][ZI][F]"
FEED_RATE_MOVE         = "[XI][YI][ZI]"
;
; End of file
;
END = "Z500R"
END = "G1X0Y0R"
END = "G49R"
END = "M05"
END = "M09"
END = "Z500R"
END = "M02"
