;
; Cipher / Mult-CAM configuration file 
; History
; Who When     What
; === ======== ========================================
; TM  modified to suit HPGL format as supplied on 08/06/95
; BEM modified to match Multicam_in which had better control of speeds etc
; BEM 06/08/02 Enabled DESCRIPTION and FILE_EXTENSION   
;
;
DESCRIPTION = "MultiCAM New -(mm) (*.plt)"
;
FILE_EXTENSION = "plt"
;
; Set units used in file - MM
;
UNITS = mm
;
; Cariage return - line feed at end of each line
; END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
FORMAT = [F|@||1.0|0.0166]
;
; Tool moves in x,y and z
; Multi-CAM uses positions 200mm = 8039 units
; ie, 8039 / 200 = 40.195
;
; BEM - latest Multicamn documents say step is 40 / mm so use that
;
; Note! negative Z axis units for positive actual movement
;
FORMAT = [X|@||1.0|40]
FORMAT = [Y|@||1.0|40]
FORMAT = [Z|@||1.0|-40]
; Home tool positions 
FORMAT = [XH|@||1.0|40]
FORMAT = [YH|@||1.0|40]
FORMAT = [ZH|@||1.0|-40]
;
; Set up program header
;
; initialise program start - HPGL, Absolute coordinates, 3d mode, tool 1
;
START = "IN;PA;ZZ1;SP1;"
;
; Program moves
;
; Set feed rate used for rapid moves 64mm/s = 3840mm/min
;
RAPID_FEED_RATE = 3840
;
FEED_RATE_CHANGE = "SF[F];"
;
RAPID_RATE_MOVE        = "PU[X],[Y],[Z];"
FIRST_FEED_RATE_MOVE   = "PD[X],[Y],[Z];"
FEED_RATE_MOVE         = "PD[X],[Y],[Z];"
;
; End of file - go home and stop spindle
;
END = "SP0;"


