;
; Mimaki configuration file 
;
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Mimaki (*.mmk)"
;
FILE_EXTENSION = "mmk"
;
; Set units used in file - MM
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
; END_OF_LINE = " [13][10]"
;
; Mimaki doesnt have a line terminator - only spaces seperate commands
;
END_OF_LINE = " "
;
; Set up default formating for variables
;
; Feed Rate
;
; Mimaki uses mm/s for output feed rate so divide by 60
; this is same as * (1/60)
;
FORMAT = [F|@||1.1|0.0166]
;
; Tool moves in x,y and z
;
; Mimaki uses positions in 0.01 of a mm
;
; NOTE: The Z Axis is reversed compared to more 'normal' machines
;
FORMAT = [X|@||1.0|100]
FORMAT = [Y|@||1.0|100]
FORMAT = [Z|@||1.0|-100]
; Home tool positions 
FORMAT = [XH|@||1.0|100]
FORMAT = [YH|@||1.0|100]
FORMAT = [ZH|@||1.0|-100]
;
; Set up program header
;
; Start spindle
START = "!MC1;"
; set XY and Z feed rates
START = "!VZ [F]; VS [F]"
; first move from home position
START = "ZM [XH] [YH] [ZH]"
;
; Set feed rate used for rapid moves 10mm/s = 600mm/min
;
RAPID_FEED_RATE = 600
;
; Set up data output on change of feed rate
;
FEED_RATE_CHANGE = "!VZ [F]; VS [F]"
;
; Program moves
;
FEED_RATE_MOVE  = "ZM [X] [Y] [Z]"
;
; End of file - go home and stop spindle
;
END = "!MC0;"
