;
; Teetz configuration file
;
;
; History
;
; Who When     What
; === ======== ========================================
; CH  22/11/02 Written
;
DESCRIPTION = "Teetz (*.plt)"
;
FILE_EXTENSION = "plt"
;
; Set units used in file - MM
;
UNITS = MM
;
; Carriage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
;
; Teetz use mm/s for output feed rate so divide by 60
; this is same as * (1/60)
;
FORMAT = [F|@||1.0|0.0166]
;
; Tool moves in x,y and z
;
; Teetz uses positions in 0.01 of a mm
;
FORMAT = [X|@||1.0|100]
FORMAT = [Y|@||1.0|100]
FORMAT = [Z|@||1.0|-100]
; Home tool positions 
FORMAT = [XH|@||1.0|100]
FORMAT = [YH|@||1.0|100]
FORMAT = [ZH|@||1.0|-100]
;
FORMAT = [XMIN|@||1.0|100]
FORMAT = [YMIN|@||1.0|100]
FORMAT = [ZMIN|@||1.0|-100]
;
FORMAT = [XMAX|@||1.0|100]
FORMAT = [YMAX|@||1.0|100]
FORMAT = [ZMAX|@||1.0|-100]
;
; Set up program header
;
; Reset all values to default except P1 and P2
;
START = "T3D;"
;
START = "R[XMIN],[YMIN],[ZMIN],[XMAX],[YMAX],[ZMAX],[XH],[YH],[ZH];"
;
; Set up data output on change of feed rate
;
FEED_RATE_CHANGE = "V[F];"
;
; Program moves
;
FEED_RATE_MOVE  = "M[X],[Y],[Z];"
;
; Tool changes
;
TOOLCHANGE = "C[T];"
;
; End of file - go home and stop spindle
;
END = "E;"
