;
; Makino configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; BEM 25/10/95 Modified from Fanuc base file
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Makino (*.mak)"
;
FILE_EXTENSION = "mak"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "%"
START = ":artcam"
START = "G91G28X0Y0Z0"
START = "G40G17G80G49"
START = "T1M6"
START = "G90G54"
START = "G05P10000"
START = "G43[ZH]H1"
START = "G0[XH][YH][S]M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[X][Y][Z]"
;
; End of file
;
END = "G28G91Z0"
END = "G49H0"
END = "G28X0Y0"
END = "M30"
