;
; Cipher / Mult-CAM configuration file 
; History
; Who When     What
; === ======== ========================================
; TM           modified to suit HPGL format as supplied on 08/06/95
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; bem 28/03/01 Retract to safez before going home
;
DESCRIPTION = "MultiCAM (mm) (*.plt)"
;
FILE_EXTENSION = "plt"
;
; Set units used in file - MM
;
UNITS = mm
;
; Cariage return - line feed at end of each line
; END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
FORMAT = [F|@||1.0|0.0166]
;
; Tool moves in x,y and z
; Multi-CAM uses positions 200mm = 8039 units
; ie, 8039 / 200 = 40.195
;
; Note! negative Z axis units for positive actual movement
;
FORMAT = [X|@||1.0|40.195]
FORMAT = [Y|@||1.0|40.195]
FORMAT = [Z|@||1.0|-40.195]
; Home tool positions 
FORMAT = [XH|@||1.0|40.195]
FORMAT = [YH|@||1.0|40.195]
FORMAT = [ZH|@||1.0|-40.195]
;
; Set up program header
;
; initialise program start
START = "IN;"
;
; Set 3D mode
START = "ZZ1;"
;
; Set home position (pen-up)
START = "PU[XH],[YH],[ZH];"
;
; Select tool (pen) 1
START = "SP1;"
;
; Set feed rate used for moves mm/s
; FEED_RATE_CHANGE = "SF[F],[F];"
;
; Set home position (pen-down)
START = "PD[XH],[YH],[ZH];"
;
; Program moves
FEED_RATE_MOVE  = "PA[X],[Y],[Z];"
;
; End of file - go home and stop spindle
;
END = "PA[X],[Y],[ZH];"
END = "PU[XH],[YH],[ZH];"
;
END = "SP0;"


