;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; Hector Henry/JVG  March/2003 Written
; Material top must be zero 
;
DESCRIPTION = "SCM Record 130-240 Xilog Plus (mm) (*.xxl)"
;
FILE_EXTENSION = "xxl"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Set up default formating for variables
;
; Feed Rate
FORMAT = [FC|#|V|1.0]
; Plunge Feed Rate
FORMAT = [FP|#|V|1.0]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.2]
FORMAT = [Y|#|Y|1.2]
FORMAT = [Z|#|Z|1.2]
FORMAT = [IA|@|I|1.2]
FORMAT = [JA|@|J|1.2]
; Tool Format
FORMAT = [T|@|T|1.0|1.0]
;
; Header Format
;
START = "H DX[XMAX] DY[YMAX] DZ[ZMATERIAL] -AB R99 *MM /DEF V10 BZ=76"

TOOLCHANGE = ""
;
; Program moves
;
RAPID_RATE_MOVE        = "xG0 [X] [Y] [Z] [T] E=TLLEN"
FIRST_FEED_RATE_MOVE   = "XL2P [X] [Y] [Z] [FC]"
FEED_RATE_MOVE         = "xL2P [X] [Y] [Z]"
;
PLUNGE_RATE_MOVE       = "xL2P [X] [Y] [Z] [FP]"
;
;
; Circular Interpolation Moves
;
FIRST_CW_ARC_MOVE      = "xA2P G=2 [X] [Y] [Z] [IA] [JA] [FC]"
CW_ARC_MOVE            = "xA2P G=2 [X] [Y] [Z] [IA] [JA]"
;
FIRST_CCW_ARC_MOVE     = "xA2P G=3 [X] [Y] [Z] [IA] [JA] [FC]"
CCW_ARC_MOVE           = "xA2P G=3 [X] [Y] [Z] [IA] [JA]"
;
END = "N X=0 Y=0"