;
; Koerner configuration file
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; GB  23/04/96 Edited from fanuc postp
; D   23/09/96 Edited by K"rner spaces between XYZ
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Koerner (*.tap)"
;
FILE_EXTENSION = "tap"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 2
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@| S|1.0]
; Feed Rate
FORMAT = [F|#| F|1.0]
; Tool moves in x,y and z
FORMAT = [X|#| X|1.4]
FORMAT = [Y|#| Y|1.4]
FORMAT = [Z|#| Z|1.4]
; Home tool positions
FORMAT = [XH|@| X|1.4]
FORMAT = [YH|@| Y|1.4]
FORMAT = [ZH|@| Z|1.4]
;
; Set up program header
;
START = "[N] (Program N100.pgm)"
START = "[N] G90"
START = "[N] G52"
START = "[N][S]"
START = "[N] G0[ZH]"
START = "[N] G0[XH][YH]"
;
; Original values
;
;START = "[N]G91G28X0Y0Z0"
;START = "[N]G40G17G80G49"
;START = "[N]T1M6"
;START = "[N]G90G54"
;START = "[N] G43[ZH]H1"
;START = "[N] G0[XH][YH][S]M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N] G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "[N] G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[N][X][Y][Z]"
;
; End of file
;
END = "[N] G0[ZH]"
END = "[N] M30"
;
; Original values
;
;END = "[N]G28G91Z0"
;END = "[N]G49H0"
;END = "[N]G28X0Y0"
;END = "[N]M30"