;
; Modelmaster configuration file for 3 axis machining with support
; for rotating (indexing) the workpiece to a specified angle
;
; History
;
; Who When     What
; === ======== ========================================
; MA  22/09/94 Feed rate variable edited to enable both F and E to be used.
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; ejp 16/03/04 Added Rotary Indexing moves
; bem 15/09/04 Changed name to say Indexer instead of Index rotate
;              job back to zero degrees at end so known position when
;              3 sided machining etc
; ejp 08/11/04 Converted for proMa PPM
; ds  05/08/05 Removed multiplier to achieve correct mmps speed values
DESCRIPTION = "proMa PPM Indexer (*.iso)"
;
FILE_EXTENSION = "iso"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
; ejp 08/11/04 Added mulitplier to make it mm/min
; ds 05/08/05 Removed multiplier to achieve correct mmps speed values
FORMAT = [F|@||1.1]
; Tool moves in x,y and z
FORMAT = [X|@||1.4]
FORMAT = [Y|@||1.4]
FORMAT = [Z|@||1.4]
; Home tool positions 
FORMAT = [XH|@||1.4]
FORMAT = [YH|@||1.4]
FORMAT = [ZH|@||1.4]
;
; Set up program header
;
START = "M03"
START = "G00 X [XH] Y [YH] Z [ZH]"
START = "G00 Z50"
START = "G00 A[AH]"
START = "G00 Y[YH]"
;
; Commands output when a rotary index takes place
;
ROTARY_A_INDEX = "G00 Z[ZH]"
ROTARY_A_INDEX = "G00 Z50"
ROTARY_A_INDEX = "G00 A[AH]"
ROTARY_A_INDEX = "G00 Y[YH]"
;
; Program moves
;
FIRST_RAPID_RATE_MOVE  = "G00 X [X] Y [Y] Z [Z]"
RAPID_RATE_MOVE        = "G00 X [X] Y [Y] Z [Z]"
FIRST_FEED_RATE_MOVE   = "G01 X [X] Y [Y] Z [Z] F [F]"
FEED_RATE_MOVE         = "G01 X [X] Y [Y] Z [Z]"
;
; End of file - rotate index back to zero degrees so that if
; doing 3 sided machining piece orientation is always obvious
;                          
END = "G00 Z [ZH]"
END = "G00 Z50"
END = "G00 A0"
END = "G00 Y[YH]"
END = "M05"
