;
; Roland MDX15 & MDX20 RDGL configuration file 
; =========================================
; Note this post will cover 3D and 2.5D cutting 
;
; History
;
; Who When     What
; === ======== ========================================
; PAT 26/09/02 Written by Patrick Thorn & Co for Delcam - ArtCam 5.5
;
DESCRIPTION = "Roland MDX15/20(*.md2)"
;
FILE_EXTENSION = "md2"
;
; Set units used in file - MM
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
;
; Roland use mm/s for output feed rate so divide by 60
; this is ame as * (1/60)
;
FORMAT = [F|@||1.1|0.0166]
;
; Tool moves in x,y and z
;
; Roland uses positions in 0.025 of a mm on MDX15/20
;
FORMAT = [X|@||1.0|40]
FORMAT = [Y|@||1.0|40]
FORMAT = [Z|@||1.0|40]
;
; Home tool positions 
FORMAT = [XH|@||1.0|40]
FORMAT = [YH|@||1.0|40]
FORMAT = [ZH|@||1.0|40]
;
; Set up program header
;
; Initialise
;
START = ";;^IN;"
;
; Switch on the spindle
;
START = "!MC1;"
;
;
; Spindle Speed is fixed at 6500rpm on the machine
;
;
; Start moving at rapid rate
;
START = "V15.0;"
;
; Relative move x0,y0 Z upto maximum height, a safety move.
; This is needed as there are no buttons on the machine to jog.
;
START = "^PR;Z0,0,162.6;"
;
; Set Absolute mode
;
START = "^PA;"
;
; Set feed rate used for rapid moves on 3D is 15mm/s = 900mm/min
;
RAPID_FEED_RATE = 900
;
; Set up data output on change of feed rate
;
FEED_RATE_CHANGE = "V[F];"
;
; Program moves
;
FEED_RATE_MOVE  = "Z[X],[Y],[Z];"
;
; End of file - go to Roland home and stop spindle
;
END = "!MC0;H;"
