;
; Khulman configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  04/07/95 Written
; BEM 20/10/96 Modified rapid move support
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Kuhlman (*.prg)"
;
FILE_EXTENSION = "prg"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.0]
; Tool moves in x,y and z
FORMAT = [X|@|X|1.4]
FORMAT = [Y|@|Y|1.4]
FORMAT = [Z|@|Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
RAPID_FEED_RATE = 2000
;
; Set up program header
;
START = " G90G0G59G40G17G191"
START = " T1M66"
START = " [S]M3"
START = " M8"
; START = "G0[ZH]H1"
START = "G0 [XH] [YH] [ZH] F2000"
;
; Program moves
;
FIRST_RAPID_RATE_MOVE  = "G0 [X] [Y] [Z] [F]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = " [X] [Y] [Z]"
;
; End of file
;
END = "G40 G0 [ZH] M9"
END = "M30"


