;
; LSI 800 XT HotWire inch configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  12/04/97 Modified Fanuc file to suite
; SP  24/11/00 Edited to suite Camtech CMC 2 machine
; SP  22/12/00 Added DESCRIPTION and FILE_EXTENSION fields
; BEM 04/07/01 Change extension to ncc (as suggested by HE) 
; GGS 21/09/05
; MD  02/13/06 Fix rounding for Mach2 bug. Y->B
;
;
;There are two version of the foam postp.  10thou and 1thou.
;Use 1thou by default (more acurate).
;Use 10thou if there are feedrate troubles when using 1thou (ie moves too fast when a 90 or 180 angle is encountered.
;
DESCRIPTION = "LSI800XTFoam INCH (*.FOA)"
;
FILE_EXTENSION = "FOA"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 1
LINE_NUM_INCREMENT = 5
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|B|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|B|1.3]
;
; Set up program header
;
; Program moves
;
RAPID_RATE_MOVE        = "G1[X][Y]F24"
FIRST_FEED_RATE_MOVE   = "G1[X][Y]F24"
FEED_RATE_MOVE         = "[X][Y]"
;
; End of file
;
