;
; Axyz configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; bmd 09/04/03 Added Arc support and changed units to INCH
; bmd 01/03/04 Added toolchange support
; bmd 13/01/05 Modified Arc Call Out/Tool Description
; tls 20/03/08 Modified to run Axyz new controller
; bmd 24/03/08 Added Toolchange Support for New Controller
; bmd 02/04/08 Added Absolute Arc Call Outs
; bmd 21/05/08 Added Line Numbers to Output Code
;
DESCRIPTION = "AXYZ_A2MC_INCH (*.nc)"
;
FILE_EXTENSION = "nc"
;
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 9999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@| N|1.0]
; Spindle Speed
FORMAT = [S|@| S|1.0]
; Feed Rate
FORMAT = [F|#| F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#| X|1.4]
FORMAT = [Y|#| Y|1.4]
FORMAT = [Z|#| Z|1.4]
; Arc Centre Cordinates
FORMAT = [IA|@| I|1.4]
FORMAT = [JA|@| J|1.4]
; Home tool positions 
FORMAT = [XH|@| X|1.4]
FORMAT = [YH|@| Y|1.4]
FORMAT = [ZH|@| Z|1.4]
;
; Set up program header
;
START = "[N]G90"
START = "[N]([TOOLDESC])"
START = "[N]M6T[T]"
START = " F0.0"
START = " F0.0"
START = "[N]M3[S]"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N]G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "[N]G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[N][X][Y][Z]"
;
FIRST_CW_ARC_MOVE      = "[N]G2[X][Y][IA][JA][F]"
CW_ARC_MOVE            = "[N]G2[X][Y][IA][JA]"
;
FIRST_CCW_ARC_MOVE     = "[N]G3[X][Y][IA][JA][F]"
CCW_ARC_MOVE           = "[N]G3[X][Y][IA][JA]"
;
;Setup Toolchange Commands
;
;
; End of file
;
;
END = "[N]M5"
END = "[N]M30"
;
TOOLCHANGE = "[N]M5"
TOOLCHANGE = "[N]G0[ZH]"
TOOLCHANGE = "[N]([TOOLDESC])"
TOOLCHANGE = "[N]M6T[T]"
TOOLCHANGE = "F0.0"
TOOLCHANGE = "F0.0"
TOOLCHANGE = "[N]M3[S]"
;