;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
; BEM 20/05/99 Removed line numbers
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Charlychangeur rotary(A) (mm) (*.iso)"
;
FILE_EXTENSION = "iso"
;
UNITS = MM
;
; Rotary axis control
;
ROTARY_AXIS = X
ROTARY_AXIS_SIGNED = NO
; if ROTARY_ORIGIN_IS_CENTRE is set to YES, the tool Z Zero position
; should ALWAYS be set to the centre of the rotary axis no matter
; what the diameter of the object being rotary machined. ArtCAM will
; compensate for the correct machining diameter specified when the
; toolpath was calculated as a rotary toolpath. If the toolpath was not
; calculated as a rotary toolpath, it will be wrapped around a cylinder
; with the circumference of the X length of the relief
;
ROTARY_ORIGIN_IS_CENTRE = YES
;
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|@|Y|1.3|-1]
FORMAT = [Y|@|X|1.3]
FORMAT = [Z|@|Z|1.3]
FORMAT = [R|@|A|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
FORMAT = [RH|@| A|1.3]
;
; Set up program header
;
START = "T[T]"
START = "[S]M3"
START = "G0[XH][YH]"
START = "G0[ZH]"
;
; Program moves
;
FIRST_RAPID_RATE_MOVE  = "G0 [Y] [Z] [R] [F]"
FIRST_FEED_RATE_MOVE   = "G1 [Y] [Z] [R] [F]"
FEED_RATE_MOVE         = "[Y] [Z] [R]"
;
; Toolchange Sections
;
TOOLCHANGE = "T[T]"
TOOLCHANGE = "[S]M3"
TOOLCHANGE = "G0[XH][YH]"
TOOLCHANGE = "G0[ZH]"
;
; End of file
;
END = "G0[ZH]"
END = "G0X0Y0"
END = "M30"
