;
; Fanuc configuration file edited to suite Bobcad 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; JAB ???????  Sent to customer to run Bobcad router(entered by sean)
; SP  10/01/01 Added DESCRIPTION and FILE_EXTENSION fields
; SP  10/01/01 Edited to suite millimeters
;
DESCRIPTION = "Bobcad_mm (*.agc)"
;
FILE_EXTENSION = "agc"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "%"
;
; Program moves
;
RAPID_RATE_MOVE        = "G00 [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "G01 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "[X] [Y] [Z]"
;
; End of file
;
END = "[ZH]"
END = "[XH] [YH]"
END = "%"