;
; Fagor 8055 configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
;
DESCRIPTION = "Motion Master Fagor8055 (*.pim)"
;
FILE_EXTENSION = "pim"
;

UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "%,ArtCAM,MX,"
START ="G90"
START ="T[T]"
START ="M6"
START ="G54"
START ="[S]M3"
START ="G4K600"
START ="G5"
START ="G0[XH][YH]"
START ="G43[ZH]D[T]"
;
; Program moves
;
RAPID_RATE_MOVE        ="G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   ="G1[X][Y][Z][F]"
FEED_RATE_MOVE         ="[X][Y][Z]"
;Setup Toolchange Commands
;
TOOLCHANGE = "M5"
TOOLCHANGE = "T[T]"
TOOLCHANGE = "M6"
TOOLCHANGE = "[S]M3"
TOOLCHANGE = "G4K600"
TOOLCHANGE = "G0[X][Y]"
TOOLCHANGE = "G43[ZH]D[T]"
;
; End of file
;
END ="M5"
END ="G53"
END ="M30"
