;
; Roland Modela configuration file 
;
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; BEM 13/05/94 Modified header to remove @ command
; TM  07/02/96 Modified - added pause command
; TM  07/02/96 Modified - Additional XY feedrates
; JAB 21/06/99 Modified for the Modela, half resolution
; TM  25/11/99 Modified to use steps of 0.25mm
; BEM 09/06/00 Added Description and file extension fields
;
DESCRIPTION = "Roland Modela (*.rol)"
;
FILE_EXTENSION = "rol"
;
; Set units used in file - MM
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Feed Rate
;
; Roland use mm/s for output feed rate so divide by 60
; this is ame as * (1/60)
;
FORMAT = [F|@||1.0|0.0166]
;
; Tool moves in x,y and z
;
; Roland uses positions in 0.01 of a mm on CAMM3
; On the Modela they use 0.025 of a mm.
;
FORMAT = [X|@||1.0|40]
FORMAT = [Y|@||1.0|40]
FORMAT = [Z|@||1.0|40]
; Home tool positions 
FORMAT = [XH|@||1.0|40]
FORMAT = [YH|@||1.0|40]
FORMAT = [ZH|@||1.0|40]
;
; Set up program header
;
; Reset all values to default except P1 and P2
;
START = "^DF"
;
; Pause before moving to start position
;
; START = "!NR"
;
; Set up Z2 to safe z (home z) - raise spindle
; move to home position and start spindle
;
;START = "@0,[ZH]M[XH],[YH]! 1"
START = "! 1;Z [XH],[YH],[ZH]"
;
; Start moving at rapid rate
;
START = "V 64;F 64"
;
; Set feed rate used for rapid moves 64mm/s = 3840mm/min
;
RAPID_FEED_RATE = 3840
;
; Set up data output on change of feed rate
;
FEED_RATE_CHANGE = "V [F];F [F]"
;
; Program moves
;
FEED_RATE_MOVE  = "Z [X],[Y],[Z]"
;
; End of file - go home and stop spindle
;
END = "H"
