;
; G - Code for Elu CNC860K
;
; History
;
; Who When     What
; === ======== ========================================
; TM  30/03/00 Written based on std g-code
; SM  12/06/00 Modified by S Merewood - CENTRAL CNC
; BEM 06/08/02 Enabled FILE_EXTENSION   
;
;
DESCRIPTION = "Elu CNC860K (mm) (*.cnc)"
;
FILE_EXTENSION = "cnc"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 2
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@||1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "PROGNAME"
START = "[N]G90"
START = "[N]G01 6"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N]G00[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "[N]G01[X][Y][Z]"
FEED_RATE_MOVE         = "[N]G01[X][Y][Z]"
;
; End of file
;
END = "[N]G00[ZH]"
END = "[N]G00X0Y0"
