;
; GRAVOGRAPH HPGL configuration file 
;
; NOTE: there are no z moves output
;
; History
; Who When     What
; === ======== ========================================95
; bem 25/09/00 Written
; bmd 14/02/05 Modified to run Gravograph 3 axis
; bmd 26/05/06 Modified to run Hermes 400 IS Engraver
;
DESCRIPTION = "Hermes 400 (*.plt)"
;
FILE_EXTENSION = "plt"
;
; Set units used in file - MM
;
UNITS = MM
;
; Cariage return - line feed at end of each line ?
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Each step is 0.025mm
;
;
FORMAT = [X|@||1.0]
FORMAT = [Y|@||1.0]
FORMAT = [Z|@||1.0]
; Home tool positions 
FORMAT = [XH|@||1.0]
FORMAT = [YH|@||1.0]
FORMAT = [ZH|@||1.0]
;
; Set up program header
;
; initialise program start
;
START = "DF"
START = "V 37"
;START = "!NR"
START = "! 1"
START = "Z 15250 10500 [ZH]"
;
;-----------------------------------------------
; Set home position (pen-up)
;START = "!MC 1;"            **Old Gravograph Start**
; Select tool (pen) 1
;START = "VS 15; !VZ 7; !PZ 55,200;"
;START = "!DR 0;"
;-----------------------------------------------
;
; Program moves
;
FEED_RATE_CHANGE = "V [F]"
;
PLUNGE_RATE_MOVE = "Z [X] [Y] [Z]"
;
;FIRST_RAPID_RATE_MOVE = "Z [X] [Y] [Z]"
RAPID_RATE_MOVE  = "Z [X] [Y] [Z]"
;
FIRST_FEED_RATE_MOVE = "Z [X] [Y] [Z]"
FEED_RATE_MOVE   = "Z [X] [Y] [Z]"
;
; End of file
;
END = "Z 0 10500 [ZH]"
END = "! 0"
END = "H"
;END = "JF"
;