;
; Anilam configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  14/11/00 Written
; BEM 31/07/01 Output FEED within [F] as if feed and plunge
;              were the same were outputing FEED on its own
;
DESCRIPTION = "Anilam (mm) (*.m)"
;
FILE_EXTENSION = "m"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|FEED |1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "DIM ABS"
START = "UNIT MM"
START = "PLANE XY"
START = "RAPID  [XH] [YH] [ZH] TOOL# 0"
START = "TOOL# [T]"
;
; Program moves
;
RAPID_RATE_MOVE        = "RAPID  [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "LINE [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "LINE  [X] [Y] [Z]"
;
; End of file
;
;END = "[ZH]"
;END = "X0.0 Y0.0 "
END = "ENDMAIN"

