;
; MultiCAM G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
; BEM 20/05/99 Removed line numbers
; SP May2/2000 Edited for Multicam
; SP May8/2000 Edited for Multicam
; bmd 02/05/08 Modified for Plasma Cutter
; tls 06/05/08 Changed G75 in startup to G74
; pah 10/10/08 Copied PLUNGE_RATE_MOVE from FIRST_PLUNGE_RATE_MOVE
;
DESCRIPTION = "MultiCAM Gcode arc Plasma (inch) (*.cnc)"
;
FILE_EXTENSION = "cnc"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|@|X|1.4]
FORMAT = [Y|@|Y|1.4]
;FORMAT = [Z|#|Z|1.4|-1]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
;FORMAT = [ZH|@|Z|1.4|-1]
;
; Arc Centre Cordinates
FORMAT = [I|@|I|1.4]
FORMAT = [J|@|J|1.4]
;
; Set up program header
;
START = "M90"
START = "G90"
START = "G74"
START = "M25"
START = "G00T1"
START = "G00[XH][YH]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G00[X][Y]"
FIRST_FEED_RATE_MOVE   = "G01[X][Y]"
FEED_RATE_MOVE         = "G01[X][Y]"
FIRST_PLUNGE_RATE_MOVE = "M11"
PLUNGE_RATE_MOVE       = "M11"
RETRACT_MOVE           = "M21"
;
FIRST_CW_ARC_MOVE      = "G02[X][Y][I][J]"
CW_ARC_MOVE            = "G02[X][Y][I][J]"
;
FIRST_CCW_ARC_MOVE     = "G03[X][Y][I][J]"
CCW_ARC_MOVE           = "G03[X][Y][I][J]"
;
; End of file
;
END = "M02"
;