;
; GIOTTO W/Fanuc configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written for std. fanuc
; PEK 05/07/00 Written for giotto, modifying std. fanuc con file.
; SH  07/07/00 modified Units in->mm .
; SH  07/07/00 TLO "H20=>H90"
; SH  07/07/00 End of file, moved M5S0 in front of G53 Y0 move
; SH  07/07/00 Program Header, added M59(hood up)
; SH  07/07/00 G52 offset modification
; PEK 28/07/00 Added toolchange and modified startup per Scotts request.
;
DESCRIPTION = "CMS Giotto(Fanuc)(*.tap)"
;
FILE_EXTENSION = "tap"
;
UNITS = mm
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "%"
START = "O3001 ([PATHNAME])"
START = "/M34"
START = "M59"
START = "M5S0"
START = "M100"
START = "M46"
START = "G53 G90 G00 Z0 H0"
START = "G17"
START = "G90"
START = "G55"
START = "[N]"
START = "G52 X0 Y0 Z0"
START = "T[T]"
START = "/T[T] M06"
START = "/M61"
START = "/M03 [S]"
START = "G0 X0 Y0"
START = "G43 Z20 H9[T]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[X][Y][Z]"
;
; Toolchange
;
TOOLCHANGE = "G53 G90 G00 Z0 H0"
TOOLCHANGE = "M5S0"
TOOLCHANGE = "T[T]"
TOOLCHANGE = "/T[T] M06"
TOOLCHANGE = "/M3[S]"
TOOLCHANGE = "G0 X0 Y0"
TOOLCHANGE = "G43 Z20 H9[T]"
;
; End of file
;
END = "G53 G90 G00 Z0 H0"
END = "M05 S0"
END = "G53 G90 G00 Y0"
END = "M46"
END = "M100"
END = "M98 P9002"
END = "M30"
END = "%"