;
; FlexiCAM configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; JON 26/12/01 Written
;
DESCRIPTION = "Flexicam (mm) (*.GC)"
;
FILE_EXTENSION = "GC"

;
UNITS = mm
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.3]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3|-1]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3|-1]
;
; Set feed rate used for rapid moves 1000in/min
;
RAPID_FEED_RATE = 1000
;
;
; Set up program header
;
START = "%"
START = "G90" 
START = "G71"
START = "G40"
START = "[S]"
START = "T[T]"
START = "G0 [XH] [YH] [F]"
START = " [ZH]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0 [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "[X] [Y] [Z]"
;
; End of file
;
END = "G0 [ZH] [F]"
END = "G0 X0 Y0"
END = "M30"
END = "M2"
END = "%"

TOOLCHANGE = "T[T]"
