;
; Pacer configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99    Copied from std Fanuc
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; tm  10/10/02 Add Arc Support
;
DESCRIPTION = "Pacer New Arcs(*.G00)"
;
FILE_EXTENSION = "G00"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Arc Centre Cordinates
FORMAT = [I|@|I|1.3]
FORMAT = [J|@|J|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "%"
START = ":1248"
START = "G91G28X0Y0Z0"
START = "G40G17G80G49"
START = "M6 T[T]"
START = "G90G54"
START = "G43[ZH]H1"
START = "[S]M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[X][Y][Z]"
;
;
FIRST_CW_ARC_MOVE      = "G2[X][Y][I][J][F]"
CW_ARC_MOVE            = "G2[X][Y][I][J]"
;
FIRST_CCW_ARC_MOVE     = "G3[X][Y][I][J][F]"
CCW_ARC_MOVE           = "G3[X][Y][I][J]"
;
;; Toolchange commands
;
TOOLCHANGE = "M06T[T]"
; TOOLCHANGE = "([TOOLDESC])"
TOOLCHANGE = "[S]M03"
; End of file
;
END = "G28G91Z0"
END = "G49H0"
END = "G28X0Y0"
END = "M30"
