; Canon Raster/PCL5e Fax Driver INF for Microsoft Windows (x86)
; Copyright CANON INC. 2013 All Rights Reserved
; CNXRPCW2.inf
; InfID: {350038B5-59E2-4379-90CC-E9365751E43F}

[Version]
Signature="$Windows NT$"
Provider=%CANON%
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
DriverVer=03/01/2013,8.90.0.0
CatalogFile=CNXRPCw2.cat
DriverIsolation=2

[Manufacturer]
%CANON%=Canon,NTx86.5.1,NTx86.6.0

[Canon]
"Canon MF4700 Series (FAX)"             =MF4700Series_FAX,USBPRINT\CanonMF4700_Series_FDA68

[Canon.NTx86.5.1]
"Canon MF4700 Series (FAX)"             =MF4700Series_FAX,USBPRINT\CanonMF4700_Series_FDA68

[Canon.NTx86.6.0]
"Canon MF4700 Series (FAX)"             =MF4700Series_FAX,USBPRINT\CanonMF4700_Series_FDA68
"Canon MF4700 Series (FAX)"             =MF4700Series_FAX,CanonMF4700_Series_FDA68
				
[MF4700Series_FAX]
CopyFiles=MF4700FC,FAX_IMG,FAX_COM,FAX_RASTER,PCOM_CS,COLOR_COM,COLOR_IMG,UTL_NC,NS_CPCA_LM3b,UTL_COM,UTL_DSP
DataFile=MF4700FC.xpd
DataSection=MF4700FC_DATA
LanguageMonitor=%NS_LMON3b_CPCA%


[OEM URLS]
%CANON% = "http://www.canon.com/support"

[MF4700FC]
MF4700FC.xpd
MF4700FC.cfg,CnFcd57K.cfg
CNFR0M_D35E2.dll,CNFR0M.dll
CNFR0MUI_D35E2.dll,CNFR0MUI.dll
CNFR0804_D35E2.dll,CNFR0804.dll
CNFRC_D35E2.chm, CNFRC.chm

[MF4700FC_DATA]
DriverFile=CNFR0M_D35E2.dll
ConfigFile=CNFR0MUI_D35E2.dll
HelpFile=CNFRC_D35E2.chm


[FAX_IMG]
CnxP0RsW.dll

[FAX_COM]
CNXADR.dll
CNXCR.dll
CNXCCR.dll
CNXDMAN.dll
CNFX0HD.dll
CNFX0IC.dll

[FAX_RASTER]
CNXP3FGU.dll
CNXP3FU3.dll
CnFX1CTS.dll
CNFX2CSV.inf
CNFX2CUA.dll
CNFX2CUA.chm
CNFX2CUC.dll
CNFX2CCS.dll
CNFX2CWS.dll
CNFX2CMS.dll

[PCOM_CS]
CPC1CS.dll
CPC10S.dll
CPC10D.exe
CPC10Q.exe
CPC10E.dll
CPC10V.exe

[COLOR_COM]
CnXPCF32.dll
CnXPCP32.dll
CNXPVT32.dll
CnXPTN32.dll
UCS32P.dll
CNLK.prf

[COLOR_IMG]
CNFXCM32.DLL
CMDFFXK.DAT

[UTL_NC]
AUSSDRV.dll

[UTL_COM]
CNXP0LOG.DLL

[NS_CPCA_LM3b]
CNAS0MOK.DLL,,,0x00000020

[UTL_DSP]
CNFXG1DS.dll

[DestinationDirs]
DefaultDestDir=66000
NS_CPCA_LM3b=66002

[SourceDisksNames.x86]
1=%DISK1%,fax.cab,

[SourceDisksFiles]
MF4700FC.xpd=1
;
CNFR0M.dll=1
CNFR0MUI.dll=1
CNFR0804.dll=1
CnxP0RsW.dll=1
;
CNFRC.chm=1
;
CNXADR.dll=1
CNXCR.dll=1
CNXCCR.dll=1
CNXDMAN.dll=1
CNFX0HD.dll=1
CNFX0IC.dll=1
;
CNXP3FGU.dll=1
CNXP3FU3.dll=1
CnFX1CTS.dll=1
CNFX2CSV.inf=1
CNFX2CUA.dll=1
CNFX2CUA.chm=1
CNFX2CUC.dll=1
CNFX2CCS.dll=1
CNFX2CWS.dll=1
CNFX2CMS.dll=1
;
CPC1CS.dll=1
CPC10S.dll=1
CPC10D.exe=1
CPC10Q.exe=1
CPC10E.dll=1
CPC10V.exe=1
;
CnXPCF32.dll=1
CnXPCP32.dll=1
CNXPVT32.dll=1
CnXPTN32.dll=1
UCS32P.dll=1
CNLK.prf=1
;
CNFXCM32.DLL=1
CMDFFXK.DAT=1
;
AUSSDRV.dll=1
;
CNXP0LOG.DLL=1
CNAS0MOK.DLL=1
;
CNFXG1DS.dll=1
CnFcd57K.cfg=1

[Strings]
CANON="Canon"
NS_LMON3b_CPCA="CPCA Language Monitor3b,CNAS0MOK.DLL"
DISK1="Canon MF4700 Series Setup Disk"
