# Static Call Graph for image C:\Users\Administrator\Desktop\模块篇 7.摄像头模块\摄像头(2.4寸、2.8寸、3.2寸驱动芯片ILI9325)(中断)\LY-STM32.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Wed Dec 03 18:04:33 2014

### Maximum Stack Usage = 104 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ FSMC_Configuration

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - Reset_Handler
  - NMI_Handler
  - HardFault_Handler
  - MemManage_Handler
  - BusFault_Handler
  - UsageFault_Handler
  - SVC_Handler
  - DebugMon_Handler
  - PendSV_Handler
  - SysTick_Handler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMA1_Channel1_IRQHandler
  - DMA1_Channel2_IRQHandler
  - DMA1_Channel3_IRQHandler
  - DMA1_Channel4_IRQHandler
  - DMA1_Channel5_IRQHandler
  - DMA1_Channel6_IRQHandler
  - DMA1_Channel7_IRQHandler
  - ADC1_2_IRQHandler
  - USB_HP_CAN1_TX_IRQHandler
  - USB_LP_CAN1_RX0_IRQHandler
  - CAN1_RX1_IRQHandler
  - CAN1_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - TIM8_BRK_IRQHandler
  - TIM8_UP_IRQHandler
  - TIM8_TRG_COM_IRQHandler
  - TIM8_CC_IRQHandler
  - ADC3_IRQHandler
  - FSMC_IRQHandler
  - SDIO_IRQHandler
  - TIM5_IRQHandler
  - SPI3_IRQHandler
  - UART4_IRQHandler
  - UART5_IRQHandler
  - TIM6_IRQHandler
  - TIM7_IRQHandler
  - DMA2_Channel1_IRQHandler
  - DMA2_Channel2_IRQHandler
  - DMA2_Channel3_IRQHandler
  - DMA2_Channel4_5_IRQHandler
  - main
  - SystemInit
  - __main

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  fputc (Thumb, 32 bytes, Stack size 16 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> USART_SendData
  - >> USART_GetFlagStatus

  NVIC_Configuration (Thumb, 124 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = NVIC_Configuration ⇒ GPIO_Init
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> GPIO_Init
  - >> GPIO_EXTILineConfig
  - >> EXTI_Init
  [Called By]
  - >> main

  USART_Configuration (Thumb, 70 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = USART_Configuration ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_ClearFlag
  [Called By]
  - >> main

  GPIO_Configuration (Thumb, 462 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  RCC_Configuration (Thumb, 72 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_Configuration ⇒ SystemInit ⇒ SetSysClock
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  - >> SystemInit
  [Called By]
  - >> main

  main (Thumb, 94 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = main ⇒ FSMC_Configuration
  [Calls]
  - >> delay_ms
  - >> ILI_9325_CLEAR
  - >> ILI9325_Init
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> FSMC_Configuration
  - >> Cmos7670_init
  - >> RCC_Configuration
  - >> GPIO_Configuration
  - >> USART_Configuration
  - >> NVIC_Configuration
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  RCC_HSE_Configuration (Thumb, 90 bytes, Stack size 8 bytes, pbdata.o(.text), UNUSED)
  [Calls]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit

  delay (Thumb, 10 bytes, Stack size 0 bytes, pbdata.o(.text))
  [Called By]

  - >> ILI9325_Init

  delay_us (Thumb, 50 bytes, Stack size 0 bytes, pbdata.o(.text))
  [Called By]

  - >> rdCmos7670Reg
  - >> WrCmos7670
  - >> I2C_Read_Byte
  - >> I2C_Send_Byte
  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Stop
  - >> I2C_Start

  delay_ms (Thumb, 52 bytes, Stack size 0 bytes, pbdata.o(.text))
  [Called By]

  - >> Cmos7670_init
  - >> main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 46 bytes, Stack size 8 bytes, stm32f10x_it.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  Get_CMOS_Data (Thumb, 158 bytes, Stack size 8 bytes, stm32f10x_it.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_CMOS_Data
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> EXTI4_IRQHandler

  EXTI4_IRQHandler (Thumb, 374 bytes, Stack size 24 bytes, stm32f10x_it.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = EXTI4_IRQHandler ⇒ Get_CMOS_Data
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_Data
  - >> LCD_WR_CMD
  - >> EXTI_ClearITPendingBit
  - >> Get_CMOS_Data
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  FSMC_Configuration (Thumb, 92 bytes, Stack size 96 bytes, stm32_fsmc.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = FSMC_Configuration
  [Calls]
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  [Called By]
  - >> main

  LCD_WR_REG (Thumb, 8 bytes, Stack size 0 bytes, lcd_ili9325.o(.text))
  [Called By]

  - >> ILI_9325_Draw_Point
  - >> EXTI4_IRQHandler

  LCD_WR_Data (Thumb, 6 bytes, Stack size 0 bytes, lcd_ili9325.o(.text))
  [Called By]

  - >> ILI_9325_Draw_Point
  - >> EXTI4_IRQHandler

  LCD_WR_CMD (Thumb, 12 bytes, Stack size 0 bytes, lcd_ili9325.o(.text))
  [Called By]

  - >> ILI_9325_Draw_Point
  - >> EXTI4_IRQHandler
  - >> ILI9325_Init

  ILI9325_Init (Thumb, 498 bytes, Stack size 8 bytes, lcd_ili9325.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ILI9325_Init
  [Calls]
  - >> LCD_WR_CMD
  - >> delay
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> main

  ILI_9325_Draw_Point (Thumb, 70 bytes, Stack size 12 bytes, lcd_ili9325.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ILI_9325_Draw_Point
  [Calls]
  - >> LCD_WR_REG
  - >> LCD_WR_Data
  - >> LCD_WR_CMD
  [Called By]
  - >> ILI_9325_CLEAR

  ILI_9325_CLEAR (Thumb, 46 bytes, Stack size 16 bytes, lcd_ili9325.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = ILI_9325_CLEAR ⇒ ILI_9325_Draw_Point
  [Calls]
  - >> ILI_9325_Draw_Point
  [Called By]
  - >> main

  I2C_GPIO (Thumb, 52 bytes, Stack size 8 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = I2C_GPIO ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> Cmos7670_init

  I2C_SDA_OUT (Thumb, 32 bytes, Stack size 8 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = I2C_SDA_OUT ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> I2C_Send_Byte
  - >> I2C_Ack

  I2C_SDA_IN (Thumb, 26 bytes, Stack size 8 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = I2C_SDA_IN ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> I2C_Read_Byte
  - >> I2C_Send_Byte

  I2C_Start (Thumb, 68 bytes, Stack size 8 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_Start
  [Calls]
  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> rdCmos7670Reg
  - >> WrCmos7670

  I2C_Stop (Thumb, 52 bytes, Stack size 8 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_Stop
  [Calls]
  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> rdCmos7670Reg
  - >> WrCmos7670

  I2C_Ack (Thumb, 66 bytes, Stack size 8 bytes, iic.o(.text), UNUSED)
  [Calls]

  - >> I2C_SDA_OUT
  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits

  I2C_NAck (Thumb, 68 bytes, Stack size 8 bytes, iic.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> rdCmos7670Reg

  I2C_Send_Byte (Thumb, 164 bytes, Stack size 16 bytes, iic.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = I2C_Send_Byte ⇒ I2C_SDA_IN ⇒ GPIO_Init
  [Calls]
  - >> I2C_SDA_IN
  - >> I2C_SDA_OUT
  - >> GPIO_ReadInputDataBit
  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> rdCmos7670Reg
  - >> WrCmos7670

  I2C_Read_Byte (Thumb, 88 bytes, Stack size 16 bytes, iic.o(.text), UNUSED)
  [Calls]

  - >> I2C_SDA_IN
  - >> GPIO_ReadInputDataBit
  - >> delay_us
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> rdCmos7670Reg

  WrCmos7670 (Thumb, 78 bytes, Stack size 16 bytes, ov7670.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = WrCmos7670 ⇒ I2C_Send_Byte ⇒ I2C_SDA_IN ⇒ GPIO_Init
  [Calls]
  - >> I2C_Send_Byte
  - >> I2C_Stop
  - >> I2C_Start
  - >> delay_us
  [Called By]
  - >> set_Cmos7670reg
  - >> Cmos7670_init

  set_Cmos7670reg (Thumb, 1316 bytes, Stack size 8 bytes, ov7670.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = set_Cmos7670reg ⇒ WrCmos7670 ⇒ I2C_Send_Byte ⇒ I2C_SDA_IN ⇒ GPIO_Init
  [Calls]
  - >> WrCmos7670
  [Called By]
  - >> Cmos7670_init

  Cmos7670_init (Thumb, 36 bytes, Stack size 8 bytes, ov7670.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = Cmos7670_init ⇒ set_Cmos7670reg ⇒ WrCmos7670 ⇒ I2C_Send_Byte ⇒ I2C_SDA_IN ⇒ GPIO_Init
  [Calls]
  - >> set_Cmos7670reg
  - >> WrCmos7670
  - >> I2C_GPIO
  - >> delay_ms
  [Called By]
  - >> main

  rdCmos7670Reg (Thumb, 100 bytes, Stack size 16 bytes, ov7670.o(.text), UNUSED)
  [Calls]

  - >> I2C_Read_Byte
  - >> I2C_Send_Byte
  - >> I2C_NAck
  - >> I2C_Stop
  - >> I2C_Start
  - >> delay_us

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 268 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> I2C_SDA_IN
  - >> I2C_SDA_OUT
  - >> I2C_GPIO
  - >> GPIO_Configuration
  - >> NVIC_Configuration

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> I2C_Read_Byte
  - >> I2C_Send_Byte
  - >> Get_CMOS_Data

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> I2C_Read_Byte
  - >> I2C_Send_Byte
  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> I2C_GPIO
  - >> EXTI4_IRQHandler
  - >> ILI9325_Init
  - >> main
  - >> GPIO_Configuration

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> I2C_Read_Byte
  - >> I2C_Send_Byte
  - >> I2C_NAck
  - >> I2C_Ack
  - >> I2C_Stop
  - >> I2C_Start
  - >> EXTI4_IRQHandler
  - >> ILI9325_Init
  - >> main

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 136 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 60 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = GPIO_EXTILineConfig
  [Called By]
  - >> NVIC_Configuration

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_HSE_Configuration

  RCC_WaitForHSEStartUp (Thumb, 48 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus
  [Called By]
  - >> RCC_HSE_Configuration

  RCC_AdjustHSICalibrationValue (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_HSE_Configuration

  RCC_ITConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 194 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 102 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 38 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  EXTI_DeInit (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 154 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text))
  [Called By]

  - >> NVIC_Configuration

  EXTI_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 34 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text), UNUSED)

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_exti.o(.text))
  [Called By]

  - >> EXTI4_IRQHandler

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART_Configuration

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 32 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART_Configuration

  USART_ITConfig (Thumb, 72 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART_Configuration

  USART_DMACmd (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler
  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler
  - >> fputc

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART_Configuration

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 50 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  FSMC_NORSRAMDeInit (Thumb, 56 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NANDDeInit (Thumb, 62 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_PCCARDDeInit (Thumb, 36 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMInit (Thumb, 224 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text))
  [Called By]

  - >> FSMC_Configuration

  FSMC_NANDInit (Thumb, 132 bytes, Stack size 12 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_PCCARDInit (Thumb, 130 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMStructInit (Thumb, 114 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NANDStructInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_PCCARDStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMCmd (Thumb, 46 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text))
  [Called By]

  - >> FSMC_Configuration

  FSMC_NANDCmd (Thumb, 86 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_PCCARDCmd (Thumb, 44 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_NANDECCCmd (Thumb, 92 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_GetECC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_ITConfig (Thumb, 128 bytes, Stack size 8 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_GetFlagStatus (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_ClearFlag (Thumb, 62 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_GetITStatus (Thumb, 64 bytes, Stack size 16 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  FSMC_ClearITPendingBit (Thumb, 68 bytes, Stack size 0 bytes, stm32f10x_fsmc.o(.text), UNUSED)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> RCC_Configuration
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 192 bytes, Stack size 0 bytes, system_stm32f10x.o(.text))
  [Called By]

  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetSysClock
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols