
        Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                          for Windows 98, Windows 98 SE


 Getting Started
 ---------------

    The Windows 98, Windows 98 SE installation CD are need to
    complete this install.


    Windows 98, Windows 98 SE Installation Procedure
    ------------------------------------------------

     1. Plug PCI Ethernet adapter into the system.

     2. Start your PC normally.  Upon power up, the system will
        indicate to you that new "PCI Ethernet Controller" hardware has
        been found. Press "Next" to be continue.

     3. Insert the driver diskette into floppy disk.

     4. Select "Search for the best driver for your device [Recommanded]".

     5. Check "Floppy disk drivers." and press "Next".

     6. The system detect the necessary driver will being
        install for the new hardware.

     7. After finishing file copying, the Windows system will ask
        you to restart the system.  Select YES to reboot.

     8. During system boot up, the operating system will automatically
        detect the PCI Fast Ethernet adapter and install the driver for
        the adapter.


    Windows 98, Windows 98 SE Installation Procedure for NDIS5 driver
    ------------------------------------------------------------------

     1. Plug PCI Ethernet adapter into the system.

     2. Start your PC normally.  Upon power up, the system will
        indicate to you that new "PCI Ethernet Controller" hardware has
        been found. Press "Next" to be continue.

     3. Insert the driver diskette into floppy disk.

     4. Select "Search for the best driver for your device [Recommanded]".

     5. Check "Specify a location" and specify the path (A:\WIN98),
        then press "Next".

     6. The system detect the necessary driver will being
        install for the new hardware.

     7. After finishing file copying, the Windows system will ask
        you to restart the system.  Select YES to reboot.

     8. During system boot up, the operating system will automatically
        detect the PCI Fast Ethernet adapter and install the driver for
        the adapter.


 Trouble Shooting
 ----------------

    1. Everything is OK in Device Manager, but network adapter still
       does't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> "Control Panel" -> "Network" -> "Identification"
       icons

    2. Everything appears to be OK but network adapter still doesn't
       function properly. Please make sure that the adapter is properly
       connected to a network device (ex: HUB) and the "connection type"
       for this adapter is set to "Auto-negotiation" or the correct
       media type. You can check it in "My Computer" -> "Control Panel"
       -> "Network" -> "Properties" icons. Select "Advanced" item.


    Driver keywords:
    ----------------

      Open "My Computer" -> "Control Pannel" -> "Network" ->
      Double click "Legend/D-Link DFE-530TX ...", Select "Advanced" item.

      Click on the "Connection Type" property selection.

         The "Value" windows will show the following selections:

         AutoSense             :The driver will auto-detect the best
                                media mode.(default)
         100Base-TX            :The driver will force the media to
                                100Base-Tx half duplex mode.
         100Base-TX Full Duplex:The driver will force the media to
                                100Base-Tx full duplex mode.
         10Base-T(Twisted Pair):The driver will force the media to
                                10Base-T half duplex mode.
         10Base-T Full_Duplex  :The driver will force the media to
                                10Base-T full duplex mode.

     Choose the appropriate setting as needed.
