
         Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Packet Driver
                          Installation Overview


 User's Guide
 ------------

    File            Description
    ------------    ----------------------------------------------------
    PCNFS.TXT       Sun PC-NFS installation document
    PCTCP.TXT       FTP PC/TCP installation document
    PDIPX.TXT       IPX SHELL installation document
    NCSA.TXT        NCSA installation document
    WINSOCK.TXT     Winsock installation document

    DEVICE = DLKFET.SYS [/option] <packet_int_no>
    DLKFET.COM [/option] <packet_int_no>

    Packet Driver Parameters:


        <packet_int_no> is the software interrupt vector number used by
                        the packet driver program, which can be from
                        96 to 128.

                        Note: <packet_int_no> can be hex or decimal
                              number.
                              hex - start with '0x'.
                                ex. >DLKFET 0x62
                              dec - start with nonzero digit.
                                ex. >DLKFET 98

        </slot=##>      is the number of assigned slot, which is from 1
                        to f.

                        Note: '##' can be hex number only.
                              ex:>DLKFET /slot=1
                                 >DLKFET /slot=2
                                 >DLKFET /slot=f

        </d>            Delay Initial - The driver program will not
                        initialize the network interface card until the
                        packet driver program is accessed by its upper
                        layer program first time.

        </w>            the /w parameter is used only in the Windows
                        environment.

        </u>            unload the driver program from memory.
                        The program will automatically search for Packet
                        driver to unload.

        </n>            NetWare conversion

     To select media type, you can use :

        </autosense>    this is the default setting. It let you be able to
                        change media without restart the driver.

        </100BaseTXFD>  Force the driver to select 100Mbps full duplex mode.

        </100BaseTX>    Force the driver to select 100Mbps half duplex mode.

        </10BaseTFD>    Force the driver to select 10Mbps full duplex mode.

        </10BaseT>      Force the driver to select 10Mbps half duplex mode.

        </flow_control> Set flow_control function.


