
           Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                   NetWare Client 32 for DOS/Windows 3.1x

 Contents
 --------
    - Getting Started
      -- Client 32 for DOSWIN

 Getting Started
 ---------------
   Client 32 for DOS/Windows 3.1x
   ------------------------------

     Method 1: Install Driver During Install
               Novell NetWare Client 32 for DOS/Windows 3.1x
     -------------------------------------------------------

     1. In DOS environment, run "INSTALL" command.

     2. Follow the installation steps of Novell NetWare Client 32.

     3. In "Select a LAN Driver Type" window, select "32-bit" LAN drivers.

     4. In "32-Bit Network Board Drivers" window, select
        "USER SPECIFIED 32 BIT DRIVER".

     5. In "Insert The Driver Disk" window, input the path
        where the LAN driver and .LDI file locate:
          ex. A:\NETWARE\32BITLAN, if floppy disk is used.

     6. Select the desired parameters, eg. SLOT number....
        and continue the installation procedure.

     7. In MS Windows environment, run "SETUP" command.

     8. In "ODI Driver Selection" window, select "32 bit" mode
        and "other Boards".

     9. Enter the path and filename of the ODI driver in "ODI Driver Path"
        window.

    10. Follow the installation setps of Novell NetWare Client 32.

    11. After the installation, a STARTNET.BAT batch file will be created.
        Please check the STARTNET.BAT file contains the right parameters.

        Content of STARTNET.BAT (for 32-bit LAN driver)
        -----------------------------------------------
        SET NWLANGUAGE=ENGLISH
        C:\NOVELL\DOSCLNT\NIOS.EXE
        LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
        LOAD C:\NOVELL\CLIENT32\CMSM.NLM
        LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
        LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_802.2 SLOT=??
        LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_802.3 SLOT=??
        LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_II    SLOT=??
        LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_SNAP  SLOT=??
        LOAD C:\NOVELL\CLIENT32\IPX.NLM           <-- Binding driver
        LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM      <-- Finding server


        Parameters supported by the DLKFET.LAN driver
        ---------------------------------------------
        SLOT     1      - Forces the driver to search for the specified board

        AUTOSENSE       - This keyword configures the adapter to conduct
                          NWay Auto-negotiation to determine the network
                          speed and the duplex mode of the network connection.

        10BASET         - Force driver to 10Mbps half duplex mode.

        10BASETFD       - Force driver to 10Mbps full duplex mode.

        100BASETX       - Force driver to 100Mbps half duplex mode.

        100BASETXFD     - Force driver to 100Mbps full duplex mode.


        Content of STARTNET.BAT (for 16-bit DOS driver)
        -----------------------------------------------
        SET NWLANGUAGE=ENGLISH
        C:\NOVELL\CLIENT32\NIOS.EXE
        C:\NOVELL\CLIENT32\LSL.COM
        C:\NOVELL\CLIENT32\N16ODI.COM
        C:\NOVELL\CLIENT32\NESL.COM
        C:\NOVELL\CLIENT32\DLKFET.COM
        LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
        LOAD C:\NOVELL\CLIENT32\PC32MLID.LAN
        LOAD C:\NOVELL\CLIENT32\TCPIP.NLM
        LOAD C:\NOVELL\CLIENT32\IPX.NLM           <-- Binding driver
        LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM      <-- Finding server


        Parameters supported by the NET.CFG for DLKFET.COM driver
        ---------------------------------------------------------
        Protocol IPX
        Bind #1

        Link Driver DLKFET
        frame Ethernet_802.3
       ;frame Ethernet_802.2
       ;frame Ethernet_II
       ;frame Ethernet_SNAP

        Protocol IPX 00 Ethernet_802.3
       ;Protocol IPX E0 Ethernet_802.2
       ;Protocol IPX 8137 Ethernet_II
       ;Protocol IPX 8137 Ethernet_SNAP

       ;Optional driver keywords:
       ;--------------------------------
        AUTOSENSE     ;Autosense media type
       ;10BaseT       ;Force the driver to select 10Mbps half duplex mode.
       ;10BaseTFD     ;Force the driver to select 10Mbps full duplex mode.
       ;100BaseTX     ;Force the driver to select 100Mbps half duplex mode.
       ;100BaseTXFD   ;Force the driver to select 100Mbps full duplex mode.

        NetWare DOS Requester
                FIRST NETWORK DRIVE = F
                NETWARE PROTOCOL = NDS BIND



       NOTE: You can run the NetWare client installation program for each
             workstation type from the CLIENT directory under SYS:PUBLIC or
             directly from the CD-ROM.


     Method 2: Install Driver After Novell NetWare Client 32 for
               DOS/Windows 3.1x is Installed
     -----------------------------------------------------------
     1. Copy the LAN driver and LDI file to the \Novell\Client32 directory,
        and use text editor to edit STARTNET.BAT file directly.


     TroubleShooting
     ---------------

        If you experience the warning messages displayed when STARTNET.BAT
        is executed, "Command Line Parameter Prompt for DLKFET" then
        follow the instructions as below:

          Change
          LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_802.3
          to
          LOAD C:\NOVELL\CLIENT32\DLKFET.LAN FRAME=ETHERNET_802.3 SLOT=1
          in STARTNET.BAT, where SLOT must be the correct value as found
          by driver.


