7

7. Copy

7.1. Basic Operations

7.1.1. Basic Operations of Copying

1. Put the manuscript into the scanner glass.

| Note: | • During copying, please do not open the cover to avoid any adverse impact on the image quality. • For information about the Media Selecting Requirements, please see Section 2.4. • For information about the Media Loading Procedures, please see Section 2.5.

2. Press Copy on the control panel and enter the copy mode.

| Note: | • When the printer is in Power Saving mode, it can be woken up only by pressing The Power Saving button or sending a print/scan job. • The printer will enter copy mode automatically with restart or startup. • For operations of selecting copies, please see Section 4.1.3.

3. Press the Start button to start copy.

7.1.2. Cancel Copy Operations

If you want to cancel the copy operation, please press Cancel button. LCD screen will prompt Cancelling...

7.2. Copy Function

7.2.1. Receipt Copy

Press this button to enter Receipt Copy mode. It is used to get high-sharpness receipt copies.

Procedures for receipt copies:

1. Press this button to flash to Receipt Copy mode, and then the area on the LCD main interface to display image quality will change to display receipt;

2. Put the receipt into the scanning platform and press the Start button. The LCD will then prompt Copying...;

3. The receipt is printed after completing the scan.

7.2.2. ID Copy

Press this button to enter ID Copy mode. It is used to copy ID cards and other two-sided certificates.

Procedures for ID Card copies:

1. Press this button to flash to ID Copy mode. The area on the main interface that displays image quality will then change to display ID Card;

2. Place the certificates on the left half of the scanning platform and press the Start button to start the scan. The LCD will then prompt Copying...;

3. After scanning the first side is completed, the LCD will display Flip ID Card: Start in the first line and Finish Scan OK in the second line;

4. If the scanning of the second side of the ID Card is required, please open the cover to flip ID Card and keep it in the same area. After pressing down Start button, LCD will prompt Copying...; After completing scan, the front back of the ID Card will be copied to the same page of the same paper;

5. If only one side is required, then press the OK button to end scanning. This time only one side of the ID Card is copied to one side of the paper.

7.3. Copy Settings

Press the Menu button to enter the menu interface. The settings of specific functions are shown in the table below:

Level I Option | Level II Option |  | Level III Option
Copy Settings | Image Quality |  | Text + image
Image
Text
Back
Contrast |  | Manual adjustment
Automatic adjustment
Back
Zoom |  | 100%
141% A5->A4
122% A5->B4
115% B5->A4
97% LTR->A4
94% A4->LTR
86% A4->B5
81% B5->A5
70% A4->A5
Manual adjustment
Back
N-in-1 |  | Close
2-in-1
4-in-1 landscape orientation
4-in-1 portrait orientation
Back
Clone copy |  | Off
2 x 2
3 x 3
4 x 4
Back