Home > Network > Advanced Network Features > Print the Network Configuration Report

### Print the Network Configuration Report

Related Models:M7206W / M7216NWA / M7256WHF
The Network Configuration Report lists the network configuration, including the network print server settings.

- Node Name: The Node Name appears on the current Network Configuration Report. The default Node Name is "BRNxxxxxxxxxxxx" for a wired network or "BRWxxxxxxxxxxxx" for a wireless network (where "xxxxxxxxxxxx" is your machine's MAC Address / Ethernet Address.)
- If the IP Address on the Network Configuration Report shows 0.0.0.0, wait for one minute and try printing it again.
- You can find your machine's settings, such as IP address, subnet mask, node name, and MAC Address on the report, for example:
  - IP address: 192.168.0.5
  - Subnet mask: 255.255.255.0
  - Node name: BRN000ca0000499
  - MAC Address: 00-0c-a0-00-04-99

1. Press MENU.
2. Do one of the following:
   - (M7256WHF)

     Press or to display the Print Reports option, and then press OK.

   - (M7206W/M7216NWA)

     Press or to display the Machine Info. option, and then press OK.

3. Press or to select the Network Config option, and then press OK.
4. Press START.

Related Information
  - Advanced Network Features
  - Access Web Based Management
  - Locate Network Settings When Using Web Based Management
  - Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

Go to top of page