;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; Hector Henry/JVG  March/2003 Written
;
DESCRIPTION = "Morbidelli Xilog Plus (mm) (*.xxl)"
;
FILE_EXTENSION = "xxl"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Set up default formating for variables
;
; Feed Rate
FORMAT = [FC|#|V|1.0]
; Plunge Feed Rate
FORMAT = [FP|#|V|1.0]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3|-1.0]
FORMAT = [IA|@|I|1.3]
FORMAT = [JA|@|J|1.3]
; Tool Format
FORMAT = [T|@|T|1.0|1.0]
;
; Header Format
;
START = "H DX[XMAX] DY[YMAX] DZ[ZMATERIAL] -AD R99 *MM /DEF"
START = "SY=1"
TOOLCHANGE = ""
;
; Program moves
;
RAPID_RATE_MOVE        = "G0 [X] [Y] [Z] [T]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [FC]"
FEED_RATE_MOVE         = "G1 [X] [Y] [Z]"
;
PLUNGE_RATE_MOVE       = "G1 [X] [Y] [Z] [FP]"
;
;
; Circular Interpolation Moves
;
FIRST_CW_ARC_MOVE      = "G2 [X] [Y] [Z] [IA] [JA] [FC]"
CW_ARC_MOVE            = "G2 [X] [Y] [Z] [IA] [JA]"
;
FIRST_CCW_ARC_MOVE     = "G3 [X] [Y] [Z] [IA] [JA] [FC]"
CCW_ARC_MOVE           = "G3 [X] [Y] [Z] [IA] [JA]"
