;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
; BEM 20/05/99 Removed line numbers
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; TM   01/05/01 Added [ ] and Filename options
; SM  11/12/01 Modified start & end
; JPT 07/07/04 Modified G57 and only 2 decimal places
;
DESCRIPTION = "Goya G-Code with arcs (mm) (*.gio)"
;
FILE_EXTENSION = "gio"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.2]
FORMAT = [Y|#|Y|1.2]
FORMAT = [Z|#|Z|1.2]
; Home tool positions 
FORMAT = [XH|@|X|1.2]
FORMAT = [YH|@|Y|1.2]
FORMAT = [ZH|@|Z|1.2]
;
; Set up program header
;
START = "[91][13]"
;
; 91 = ASCII for [
; 13 10 = ASCII for Carriage return
; 93 = ASCII for ]
;
START = "[34][FILENAME][34]"
;
; 34 = ASCII for "
;
START = "G57,2"
START = "G64"
START = "G90"
START = "[S]"
START = "G68 P0"
START = "G04 F5"
START = "G00[ZH]"
START = "G00[XH][YH]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G00[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G01[X][Y][Z][F]"
FEED_RATE_MOVE         = "[X][Y][Z]"
;
FIRST_CW_ARC_MOVE      = "G02[X][Y]I[IA]J[JA]"
CW_ARC_MOVE            = "G02[X][Y]I[IA]J[JA]"
;
FIRST_CCW_ARC_MOVE     = "G03[X][Y] [IA] [JA]"
CCW_ARC_MOVE           = "G03[X][Y] [IA] [JA]"
;
; End of file
;
END = "G00[ZH]"
END = "G00X0Y0"
END = "G67 P0"
END = "M02"
END = "[93]"
;
; 93 = ASCII for ]
