;
; Prolight 1000 (G - Code) configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
; BEM 20/05/99 Removed line numbers
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; tls 03/03/05 Altered to run Prolight 1000
;
DESCRIPTION = "Prolight 1000 (inch) (*.nc)"
;
FILE_EXTENSION = "nc"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.4]
FORMAT = [Y|#|Y|1.4]
FORMAT = [Z|#|Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
;
; Set up program header
;
START = "[N]G0[ZH]"
START = "[N]G0[XH][YH][S]M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N]G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "[N]G1[X][Y][Z][F]"
FEED_RATE_MOVE         = "[N][X][Y][Z]"
;
; End of file
;
END = "[N]G0[ZH]"
END = "[N]G0X0Y0M5"
END = "[N]M2"
