;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
; BEM 20/05/99 Removed line numbers
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; jvg 26/10/05 ajusted for Techno-Isel RG Series 5950
;
DESCRIPTION = "Techno-Isel RG (inch) (*.nc)"
;
FILE_EXTENSION = "nc"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#| X|1.4]
FORMAT = [Y|#| Y|1.4]
FORMAT = [Z|#| Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
;
; Set up program header
;
START = "%"
START = "G20"
START = "G0 G17 G40 G49 G80 G90"
START = "T[T]M6"
START = "G0 [ZH]"
START = "G0 [XH] [YH] [S] M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G1[X][Y][Z] [F]"
FEED_RATE_MOVE         = "[X][Y][Z]"
;
TOOLCHANGE = "G0 [ZH]"
TOOLCHANGE = "T[T]M6"
TOOLCHANGE = "[S] M3"
;
; End of file
;
END = "G0[ZH]"
END = "M5"
END = "M30"
END = "%"
