;
; Newing Hall Apex 1+2 configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; srm 28/03/97 modified from newing
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; bem 01/08/02 Move up after initial setting at 0,0,0
;
DESCRIPTION = "Apex (*.cnc)"
;
FILE_EXTENSION = "cnc"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0|0.0033]
; Feed Rate
;
;NOTE PERCENT CALC AT END OF LINE
;
FORMAT = [F|#|F|1.1|0.01666]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.2]
FORMAT = [Y|#|Y|1.2]
FORMAT = [Z|#|Z|1.2|-1.0]
; Home tool positions 
FORMAT = [XH|@|X|1.2]
FORMAT = [YH|@|Y|1.2]
FORMAT = [ZH|@|Z|1.2|-1.0]
;
; Set up program header
;
START = "G71"
START = "G90"
START = "G00X0.00Y0.00Z0.00"
START = "M03[S]"
START = "G00X0.00Y0.00[ZH]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G00[X][Y][Z]"
FIRST_FEED_RATE_MOVE   = "G01[X][Y][Z][F]"
FEED_RATE_MOVE         = "G01[X][Y][Z][F]"
;
; End of file
;
END = "M05"
END = "M02"

