;
; Bostomatic configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; bjs 02/07/97 WRITTEN  atg
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
; bem 16/05/00 Created this inch version for testing against incremental post
;
;
DESCRIPTION = "Bostomatic Inch (*.tap)"
;
FILE_EXTENSION = "tap"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 1
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.4]
FORMAT = [Y|#|Y|1.4]
FORMAT = [Z|#|Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
;
; Set up program header
;
START = "%"
START = "G40G90G49R"
; bem - I put this in - doesnt seem to be a unit swith in mm ?
START = "G70"
START = "G01X0Y0Z100.R"
START = "T1"
START = "G48R"
START = "G01[XH][YH][S]M04R"
START = "G04X4.0"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N]G01[X][Y][Z]R"
FIRST_FEED_RATE_MOVE   = "[N]G01[X][Y][Z][F]"
FEED_RATE_MOVE         = "[N][X][Y][Z]"
;
; End of file
;
END = "Z100.R"
END = "G01X0Y0R"
END = "G49R"
END = "M05"
END = "M09"
END = "Z100.R"
END = "M02"
