;
; Northwood Toolchanger configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; BEM 01/04/94 Written
; SP  07/27/00 Edited to suite Northwood Router
; SP  07/28/00 Edited to suite Northwood Router w/toolchanger
; bmd 06/08/03 Edited to suite Northwood Router w/ Fanuc control
;
DESCRIPTION = "Northwood_Fanuc (*.txt)"
;
FILE_EXTENSION = "txt"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.4]
FORMAT = [Y|#|Y|1.4]
FORMAT = [Z|#|Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
;
; Set up program header
;
START = "%"
START = ":[FILENAME]"
START = "M98 P8000"
START = "G90"
START = "T1[T]"
START = "[S]"
START = "M98 P8101 ([TOOLDESC])"
START = "G43 H[T] G0 [ZH]"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0 [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "[X] [Y] [Z]"
;
; Setup Toolchange commands
;
TOOLCHANGE = "G90"
TOOLCHANGE = "T1[T]"
TOOLCHANGE = "[S]"
TOOLCHANGE = "M98 P8101 ([TOOLDESC])"
TOOLCHANGE = "G43 H[T] G0 [ZH]"
TOOLCHANGE = "G0[X][Y][Z]"
;

; End of file
;
END = "M98 P8001"
END = "M2"
END = "%"

