;
; Weeke configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; JWC 09/13/01 Written
; TLS 03/07/05 ZSIZE VARIABLE CHANGED TO ZMATERIAL 
;
DESCRIPTION = "Weeke MPR(*.mpr)"
;
FILE_EXTENSION = "mpr"
;

UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]

;
; Set up program header
;
START = "[91]H"
START ="VERSION=[34]4.0 Alpha[34]"
START ="MAT=[34]WEEKE[34]"
START =" "
START ="[91]001"
START ="L=[34][XSIZE][34]"
START ="KM=[34]length of workpiece[34]"
START ="W=[34][YSIZE][34]"
START ="KM=[34]width of workpiece[34]"
START ="T=[34][ZMATERIAL][34]"
START ="KM=[34]thickness of workpiece[34]"
START =" "
START = "<100 \WerkStck\"
START = "LA=[34]L[34]"
START = "BR=[34]W[34]"
START = "DI=[34]T[34]"
START =" "
START ="<119 \Polygonzug\"
START ="NM=[34][FILENAME].PLY[34]"
START ="XA=[34]L/2[34]"
START ="YA=[34]W/2[34]"
START ="BR=[34][XSIZE][34]"
START ="HE=[34][YSIZE][34]"
START ="WI=[34]0[34]"
START ="TI=[34]0[34]"
START ="WZ=[34]1[34]"
START ="RK=[34]NOWRK[34]"
START ="F_=[34]5[34]"
START ="HP=[34]0[34]"
START ="SP=[34]0[34]"
START =" "
START ="!"

;
; Program moves
;
RAPID_RATE_MOVE        =""
;"G0[X][Y][Z]"
FIRST_FEED_RATE_MOVE   =""
;"G1[X][Y][Z][F]"
FEED_RATE_MOVE         =""


