;
; Weeke PLY configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; JWC 09/13/01 Written
;
DESCRIPTION = "Weeke PLY (*.ply)"
;
FILE_EXTENSION = "ply"
;

UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|@|X|1.3]
FORMAT = [Y|@|Y|1.3]
FORMAT = [Z|@|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
; Tool Number
FORMAT = [T|#||02.0]
;
; Set up program header
;
START = "SIZE X[XSIZE] Y[YSIZE]"
START ="U"
START ="[XH] [YH]"
START ="[ZH]"
START ="D"

;START ="T[T]"
;START ="M6"
;START ="G54"
;START ="[S]M3"
;START ="G0[XH][YH]"
;START ="G43[ZH]D[T]"
;
; Program moves
;
;FIRST_RAPID_RATE_MOVE  ="[X] [Y] [13][10] [Z]"
RAPID_RATE_MOVE        ="[X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   ="[X] [Y] [Z]"
FEED_RATE_MOVE         ="[X] [Y] [Z]"
;Setup Toolchange Commands 
;
;TOOLCHANGE = "M5"
;TOOLCHANGE = "T[T]"
;TOOLCHANGE = "M6"
;TOOLCHANGE = "[S]M3"
;TOOLCHANGE = "G4K600"
;TOOLCHANGE = "G0[X][Y]"
;TOOLCHANGE = "G43[ZH]D[T]"
;
; End of file
;
;END ="M5"
;END ="G53"
;END ="M30"
END ="U"


