;
; MBP2030 configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; MSB 03/06/97 Written
; JAB 10/04/03 Edited for Cavalera - Isel Gcode
; JAB 10/04/03 Edded Arc Support
;
DESCRIPTION = "TECHNO-ISEL Arcs (*.ncd)"
;
FILE_EXTENSION = "ncd"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 0
LINE_NUM_INCREMENT = 10
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.0]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.3]
FORMAT = [Y|#|Y|1.3]
FORMAT = [Z|#|Z|1.3]
; Home tool positions 
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
FORMAT = [Radius|@|R|1.3]
;
; Set up program header
;
START = "G90"
START = "G0 [ZH]"
START = "G0 [XH] [YH]"
START = "M3"
;
; Program moves
;
RAPID_RATE_MOVE        = "G0 [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "[X] [Y] [Z]"
;
;
FIRST_CW_ARC_MOVE      = "G2 [X] [Y] [Radius]"
CW_ARC_MOVE            = "G2 [X] [Y] [Radius]"
;
FIRST_CCW_ARC_MOVE     = "G3 [X] [Y] [Radius]"
CCW_ARC_MOVE           = "G3 [X] [Y] [Radius]"
;
; End of file
;
END = "M5"
END = "M30"
