; 
;
;****PLEASE GO THROUGH THE NOTE BELOW TO USE THIS POST****
; Note: The reference point for the machine is fixed at the bottom left corner,
; hence Origin/Model Position should be set to Bottom Left Corner of ArtCAM file.  
; In the nc output the operator needs to feed in the offset from X and Y axis manually(Denoted by VX and VY in the post)  
;
; History
;
; Who When     What
; === ======== ========================================
; TRB 01/31/02 Written
; TRB 02/18/02 changed Radii and toolchange sections
; XPKUR 12/07/07 Post for WEDKIN VX confirmed by Delcam Middle East
;
DESCRIPTION = "Wedkin (*.nc)"
;
FILE_EXTENSION = "nc"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering
;
LINE_NUM_START     = 1
LINE_NUM_INCREMENT = 1
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.2]
FORMAT = [Y|#|Y|1.2]
FORMAT = [Z|#|Z|1.2]
;
; Arc Center
FORMAT = [R|@|R|1.3]
;
; Home tool positions
FORMAT = [XH|@|X|1.3]
FORMAT = [YH|@|Y|1.3]
FORMAT = [ZH|@|Z|1.3]
;
; Set up program header
;
START = "START"
START = "(DFS,P1,APS.M,RWED)"
START = "[N] VX=  VY= "
START = "[N] M79"
START = "[N] M38"
START = "[N] G0 Z0 T00"
START = "[N] M50"
START = "[N] M52"
START = "[N] [S] M3"
START = "[N] M65"
START = "[N] $99 M0"
START = "[N] (PRESS CYCLE START)"
START = "[N] M54"
START = "[N] M56"
START = "[N] G90 M38"
START = "[N] M62"
START = "[N] G53"
START = "[N] G39"
START = "[N] G0 Z0 T00"
START = "[N] G820"
START = "[N] T0[T] M8"

;
; Program moves
;
RAPID_RATE_MOVE        = "[N] G0 [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "[N] G1 [X] [Y] [Z] [F]"
FEED_RATE_MOVE         = "[N] [X] [Y] [Z]"
;
;
; Arc Section
;
FIRST_CW_ARC_MOVE      = "[N] G2 [X] [Y] R-[Radius] [F]"
CW_ARC_MOVE            = "[N] G2 [X] [Y] R-[Radius]"
;
FIRST_CCW_ARC_MOVE     = "[N] G3 [X] [Y] R-[Radius] [F]"
CCW_ARC_MOVE           = "[N] G3 [X] [Y] R-[Radius]"
;
;
;
; Toolchange Sections

; End of file
;

END = "[N] G53 M38"
END = "[N] G0 Z0 T00 M9"
END = "[N] M69"
END = "[N] G53 T00 M38"
END = "[N] X600 Y900 Z0"
END = "[N] M55"
END = "[N] M57"
END = "[N] M61"
END = "[N] G24 P99"
END = "[N] M30"

