;
; G - Code configuration file - with Arc Support
;
; History
;
; Who When     What
; === ======== ========================================
; TM  13/05/99 Written
;
DESCRIPTION = "DynaPath (inch) (*.NCC)"
;
FILE_EXTENSION = "NCC"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
; Block numbering 
;
LINE_NUM_START     = 1
LINE_NUM_INCREMENT = 1
LINE_NUM_MAXIMUM   = 999999
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@|N|1.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Tool Number
; FORMAT = [T|@|T|2.0]
; Feed Rate
FORMAT = [F|#|F|1.1]
; Tool moves in x,y and z
FORMAT = [X|#|X|1.4]
FORMAT = [Y|#|Y|1.4]
FORMAT = [Z|#|Z|1.4]
; Home tool positions 
FORMAT = [XH|@|X|1.4]
FORMAT = [YH|@|Y|1.4]
FORMAT = [ZH|@|Z|1.4]
;
; Set up program header
;
START = "(1)$"
START = "[N](9)T0[T]0[T]M6E0$"
START = "[N](9)M9$"
START = "[N](9)M03[S]$"
START = "[N](0)X0Y0$"
START = "[N](9)M8$"
START = "[N](0)[ZH]$"
;
; Program moves
;
RAPID_RATE_MOVE        = "[N](0)[X][Y][Z]$"
;
FIRST_FEED_RATE_MOVE   = "[N](1)[X][Y][Z][F]$"
FEED_RATE_MOVE         = "[N](1)[X][Y][Z][F]$"
;
; Toolchange
;
TOOLCHANGE = "[N](9)M9$"
TOOLCHANGE = "[N](9)T0[T]0[T]M6E0$"
TOOLCHANGE = "[N](9)M03[S]$"
TOOLCHANGE = "[N](0)X0Y0$"
TOOLCHANGE = "[N](9)M8$"
TOOLCHANGE = "[N](0)[ZH]$"
;
;
; End of file
;
END = "[N](9)M30$"
END = "END$"

